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Model: [model or part number]
Version [1.0], [date]
[Company name] · [website] · [support email or phone]


Before you start
Safety
1. Read every step before you start.
1. [Keep small parts away from children under three: they are a choking hazard.]
1. Two people are needed for steps [x] to [y].
1. Wear gloves when handling [part]: its edges are sharp.
1. Don't tighten the fixings fully until step [x].
Time
About [30] minutes, [one or two] people.
Tools you need
	Tool
	Size

	[Hex key]
	[4 mm, supplied]

	[Cross-head screwdriver]
	[No. 2]

	[Spanner]
	[10 mm]


Parts
Check that you have every part before you start.
	Ref
	Picture
	Part
	Qty

	A
	
	[Base panel]
	[1]

	B
	
	[Side panel]
	[2]

	C
	
	[Shelf]
	[1]

	D
	
	[Back panel]
	[1]

	E
	
	[Hinge]
	[2]

	F
	
	[Handle]
	[1]


Fixings
	Ref
	Picture
	Fixing
	Qty

	1
	
	[M4 × 12 mm screw]
	[8]

	2
	
	[M4 washer]
	[8]

	3
	
	[Wooden dowel, 8 × 30 mm]
	[4]




Step 1
	[Picture for step 1: only the parts this step adds, highlighted]


Parts: [A × 1, B × 2, 3 × 4]
[Push the dowels (3) into the holes in the base (A), then fit the two side panels (B) onto them.]
Check: [The sides stand square to the base.]
Step 2
	[Picture for step 2: only the parts this step adds, highlighted]


Parts: [C × 1, 1 × 4, 2 × 4]
[Slide the shelf (C) between the sides and fix it with four screws (1) and washers (2).]
Check: [The shelf is level and doesn't rock.]


Step 3
	[Picture for step 3: only the parts this step adds, highlighted]


Parts: [D × 1]
[Lay the unit on its front and slot the back panel (D) into the grooves.]
Check: [The back panel sits fully in its grooves.]
Step 4
	[Picture for step 4: only the parts this step adds, highlighted]


Parts: [E × 2, 1 × 4, 2 × 4]
[Fix the hinges (E) to the side panel with the remaining screws (1) and washers (2).]
Check: [The door opens and closes without catching.]


Step 5
	[Picture for step 5: only the parts this step adds, highlighted]


Parts: [F × 1]
[Screw the handle (F) on from the inside of the door.]
Check: [The handle doesn't turn.]
Step 6
	[Picture for step 6: only the parts this step adds, highlighted]


Parts: [ ]
[Tighten every fixing fully.]
Check: [Nothing moves when you push the unit from the side.]


When you've finished
Final checks
1. [Every fixing is tight.]
1. [No parts or fixings are left over.]
1. [The product stands level and doesn't rock.]
1. [Fix it to the wall with the bracket supplied, if the instructions say so.]
Care
[How to clean it, what to check now and then, and what not to do with it.]
Help
Missing or damaged parts? Contact [company] at [email or phone] with the model number above. Please don't take the product back to the shop before contacting us.
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