[WI-0001] · Rev. [A] · [Fit the motor to the gearbox]
Work instruction
[Fit the motor to the gearbox]
	Document no.
	[WI-0001]
	Revision
	[A]

	Product / part no.
	[Product name, part number]
	Effective date
	[date]

	Station / cell
	[Station or cell]
	Takt / cycle time
	[x] minutes

	Prepared by
	[name]
	Approved by
	[name, role]


Purpose and scope
Purpose: [What this instruction is for, and the result when it is done right.]
Scope: [Which products, models and stations it covers, and which it doesn't.]
Safety
1. [Wear safety glasses and gloves at this station.]
1. [Isolate the air supply before working on the press.]
1. [Lift parts over 20 kg with the hoist, not by hand.]
1. [Report any damaged tool or part to the team leader before carrying on.]
Personal protective equipment: [Safety glasses, cut-resistant gloves, safety boots]
Tools, equipment and settings
	Tool or equipment
	Setting
	Note

	[Torque driver]
	[2.5 N·m]
	[Calibrated, in date]

	[Hex key]
	[4 mm]
	[ ]

	[Press fixture]
	[Fixture no. F-12]
	[ ]


Parts and materials
	Item
	Part no.
	Description
	Qty

	1
	[PN-1001]
	[Gearbox housing]
	[1]

	2
	[PN-1002]
	[Motor]
	[1]

	3
	[PN-2001]
	[M4 × 12 socket cap screw]
	[4]

	4
	[PN-2002]
	[M4 spring washer]
	[4]




Steps
	Step
	Picture
	What to do

	1
	[Picture for step 1: the parts this step uses, highlighted. If you have the CAD model as a STEP file, lineplate.com draws these for you.]
	[Place the gearbox housing (1) in the fixture, output shaft facing down.]
Key point: [The housing sits flat on all three locating pins.]
Check: [Housing doesn't rock.]

	2
	[Picture for step 2]
	[Offer the motor (2) to the housing, aligning the shaft key with the coupling slot.]
Key point: [Don't force it: turn the shaft slightly until the key drops in.]
Check: [Motor face is flush with the housing.]

	3
	[Picture for step 3]
	[Fit the four screws (3) with washers (4), finger tight, then torque in a cross pattern.]
Key point: [Torque to 2.5 N·m, in two passes.]
Check: [All four screws marked with paint pen after torquing.]

	4
	[Picture for step 4]
	[Turn the output shaft by hand through two full turns.]
Key point: [It turns smoothly, with no tight spots or noise.]
Check: [Record pass or fail on the traveller.]




Quality checks
1. [All fixings torqued and marked.]
1. [No damage to the housing or the motor cable.]
1. [Output shaft turns freely by hand.]
1. [Serial number recorded on the traveller.]
If something is wrong
[If a check fails: stop, tag the unit with a red tag, put it in the quarantine area and tell the team leader. Don't rework it unless this instruction says how.]
Revision history
	Rev.
	Date
	Change
	By

	[A]
	[date]
	[First issue]
	[name]


Training sign-off
	Role
	Name
	Signature
	Date

	Operator trained
	[name]
	[signature]
	[date]

	Trainer
	[name]
	[signature]
	[date]
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